\subsection{DAC Motor}
\textit{Platforms: All}

\ \newline
This driver is used to control an MX analog output device as if it were
a motor.  The type of control supported here is fairly basic.  When a move
is commanded, all that happens is that the DAC output voltage is changed
to the value corresponding to the new position.

There is only one driver specific specific field for the \textit{dac\_motor}
driver.  Here is the description of it:

\ \newline
\newcommand{\MxFieldDacZmotorDacZrecord}
{The name of the MX analog output record used by this motor record.}
%
\MxDacZmotorDriverFields

