\section{EPICS Analog Input}
%
\textit{Module: \bf{epics.mxo}}
\newline

An MX \textit{epics\_ainput} record is used to read values from a
single EPICS PV.  Typically this PV is used to report a floating point value.
Optionally, it is possible to also specify the name of an additional PV
that is used to contain a dark current value for the first PV.

\ \newline
\MxEpicsZainputDriverFields
\newline

