\section{EPICS CCD}
%
\textit{Module: \bf{epics.mxo}}
\newline

An MX \textit{epics\_ccd} record is used to operate an
area detector controlled by the obsolete EPICS CCD record.
Most of these detectors have now been converted to the new
EPICS Area Detector record, but if you have one that still
uses the old driver, this is a way to use it from MX.

\ \newline
\MxEpicsZccdDriverFields
\newline

