\section{Stanford Research Systems SR-630 Thermocouple Controller}

The SR-630 is a 16-channel thermocouple readout controller which can be
used via RS-232 or GPIB.  In addition to reading thermocouple temperatures,
the SR-630 can also control voltage outputs.

There are three different MX drivers for the SR-630 controller.
The \textit{sr630} driver manages the controller as a whole.
The \textit{sr630\_ainput} driver manages a single thermocouple input.
The \textit{sr630\_aoutput} driver manages a single voltage output.

\textbf{sr630\_ainput} fields:
\newline
\MxSrGDAZainputDriverFields
\newline

\textbf{sr630\_aoutput} fields:
\newline
\MxSrGDAZaoutputDriverFields
\newline

An example database for the SR-630 looks like:
\begin{verbatim}
sr630_rs232 interface rs232 tty "" "" 9600 8 N 1 N 0x0a 0x0a 10 0x0 /dev/ttyS7
sr630 interface controller sr630 "" "" sr630_rs232
temp1  device analog_input sr630_ainput "" "" 0 1 0 C 0x0 0 "" sr630 1
temp2  device analog_input sr630_ainput "" "" 0 1 0 C 0x0 0 "" sr630 2
temp3  device analog_input sr630_ainput "" "" 0 1 0 C 0x0 0 "" sr630 3
temp4  device analog_input sr630_ainput "" "" 0 1 0 C 0x0 0 "" sr630 4
temp5  device analog_input sr630_ainput "" "" 0 1 0 C 0x0 0 "" sr630 5
temp6  device analog_input sr630_ainput "" "" 0 1 0 C 0x0 0 "" sr630 6
temp7  device analog_input sr630_ainput "" "" 0 1 0 C 0x0 0 "" sr630 7
temp8  device analog_input sr630_ainput "" "" 0 1 0 C 0x0 0 "" sr630 8
temp9  device analog_input sr630_ainput "" "" 0 1 0 C 0x0 0 "" sr630 9
temp10 device analog_input sr630_ainput "" "" 0 1 0 C 0x0 0 "" sr630 10
temp11 device analog_input sr630_ainput "" "" 0 1 0 C 0x0 0 "" sr630 11
temp12 device analog_input sr630_ainput "" "" 0 1 0 C 0x0 0 "" sr630 12
temp13 device analog_input sr630_ainput "" "" 0 1 0 C 0x0 0 "" sr630 13
temp14 device analog_input sr630_ainput "" "" 0 1 0 C 0x0 0 "" sr630 14
temp15 device analog_input sr630_ainput "" "" 0 1 0 C 0x0 0 "" sr630 15
temp16 device analog_input sr630_ainput "" "" 0 1 0 C 0x0 0 "" sr630 16
\end{verbatim}
