\subsection{XAFS Wavenumber}

This MX pseudomotor driver controls another MX motor in units of
XAFS electron wavenumber.

The XAFS electron wavenumber $k$ is computed using the equation:
$$
E_{photon} = E_{edge} + {{\hbar^2 k^2}\over{2 m_{electron}}}
$$

