\subsection{National Instruments ValueMotion}
%
\textit{Platform: Windows}
\newline

The National Instruments ValueMotion series of motor controllers uses
the MX \textit{pcmotion32} series of drivers.
The \textit{pcmotion32} family of MX drivers has two drivers:
\newline\newline
\textbf{pcmotion32} driver
\newline\newline
This driver communicates with the PCMOTION32.DLL library provided
by National Instruments.

\ \newline
\textbf{pcmotion32\_motor} driver
\newline

Here is an example database for the \textit{pcmotion32} family of
MX drivers.
\begin{verbatim}
nulogic interface controller pcmotion32 "" "" 1  0  0
m1      device motor pcmotion32_motor "" "" 0 0 -20000000 20000000 0 -1 -1 0.0001 0 um nulogic 1 20000 500 10000 1 0 0
m2      device motor pcmotion32_motor "" "" 0 0 -20000000 20000000 0 -1 -1 0.0001 0 um nulogic 2 2000 500 10000 1 0 0
\end{verbatim}
